**Raspberry Pi Set up for Profile Node:**

Step 1: Flash Raspbian Jessie into SD card using Win32DiskImager

Step 2: Plug in Raspberry Pi (with SD card) and switch on connecting it to a LCD Screen

Step 3: sudo apt-get update && sudo apt-get dist-upgrade

Step 4: clone file from github (Refer to github documentation)

Step 5: Enable SSH, SPI and I2C in sudo raspi-config.